|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **HAZARD**  | **EXPECTED OUTCOME**  | **WHO IS AFFECTED?**  | **RISK BEFORE**  | **ACTION TAKEN**  | **RISK AFTER**  |
| Over enthusiastic participants  | Minor injury, bruising, abrasions.  | Participant and staff.  | M  | Responsible person supervising at all times. In the event of large numbers of participants, extra so far should be in place. We recommend one at the base.  | L  |
| Danger of unnecessary injury  | Serious injury, bruising, abrasions.  | Participants  | M  | Ensure that no one with a history of back or neck problems or who suffers from a heart complaint use the inflatable or anyone who is feeling unwell or suffering the fact alcohol or drugs pregnant women may not use the equipment at any time.  | L  |
| Overloading or tipping over  | Minor injury, bruising, abrasions.  | Participants and staff.  | M  | No user weighing over 90 kg or 14 stone is committed to use the equipment at any time. Running from side to side is strictly forbidden. Supervisor should be used to ensure adequate adherence to weight and participant limit.  | L  |
| Danger of injury from hard surfaces  | Injury, bruising, abrasions.  | Participants  | M  | Inflatable must never be mounted unless the inflatable bed is fully inflated whether the inflatable is an operation or not this can lead to serious injury.  | L  |
| Injury through lack of supervision  | Minor injury, bruising, abrasions  | Participants  | M  | A fully trained operator must be present with the equipment at all times, in the event the operator is not in view do you not to enter any circumstance. The equipment should be switched off when no supervision is available  | L  |
| Tripping over anchorage points, spare equipment, electrical cables  | Injury, bruising, abrasions.  | Participants and staff  | H  | Anchor point to use as per manufacturer’s instructions and spare equipment erected safely or stayed away. Where possible electrical cable does not cross any public pathway. In the event of large numbers of participants attending, safety fencing should be erected  | L  |
| Tripping over bungee cords and twanging effects  | Injury, bruising, abrasions.  | Participant  | M  | Responsible person supervising at all times. Do not allow participants to be stretched along the bungee by third parties  | L  |
| Bungee cords breaking or coming on attach from anchor points or belts.  | Injury, bruising, abrasions.  | Participant, spectator and stuff  | M  | Person supervising at all times. All and points are checked at regular intervals and I’ll safety tested every 12 months. Cords are whipped at each end and to attached the inflatable  |